This zip file contains the MOHID Studio workspace (OWS) for the integrated urban flood modelling covering the pilot area of Sacavém. It includes all the model project and configurations needed.

The model application uses the numerical engines SWMM for the 1D (underground pluvial drainage network and open channels like small rivers) and MOHID Land for the 2D surface runoff model - the floodplain and Trancão river. 

it doesn't include model implemented for spain, because we are still waiting for more configuration data from the stakeholders. If no data is provided in the upcoming weeks, we will include here the eisting model "as it is".
 
